[Contents] [Prev] [Next] [Index] [Report an Error]

# mirror disable

#### Syntax

mirror disable triggerType triggerValue

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
nas-port-id added in JUNOSe Release 7.1.0.

#### Description

Disables a packet mirroring session that was dynamically configured for a subscriber; uses the trigger information to identify the subscriber's session. There is no no version.

#### Options

- triggerType—One of the following RADIUS attributes that was used as the trigger to start the packet mirroring session
  - acct-session-id—Acct-Session-Id, RADIUS attribute [44]
  - calling-station-id—Calling-Station-Id, RADIUS attribute [31]
  - ip-address—Framed-IP-Address, RADIUS attribute [8]; associated with the virtual router where the command is issued, RADIUS VSA [26-1]
  - nas-port-id—NAS-Port-Id, RADIUS attribute [87]
  - username—User-Name, RADIUS attribute [1]; associated with the virtual router where the command is issued, RADIUS VSA [26-1]
- triggerValue—Value of the triggerType (the specified RADIUS attribute) that identifies the subscriber

#### Mode

Privileged Exec

#### Related Topics

- Configuring CLI-Based Mirroring
- Configuring RADIUS-Based Mirroring

[Contents] [Prev] [Next] [Index] [Report an Error]