[Contents] [Prev] [Next] [Index] [Report an Error]

# Example: Configuring a PPPoE Subinterface for a LAG Bundle

The following example displays LACP configuration for two Fast Ethernet interfaces in slot 4. The interfaces are enabled for passive LACP. The speed and duplex characteristics are the same for both interfaces.

`

host1(config)#interface fastEthernet 4/0
host1(config-if)#speed 100
host1(config-if)#duplex full
host1(config-if)#lacp passive
host1(config-if)#interface fastEthernet 4/3
host1(config-if)#speed 100
host1(config-if)#duplex full
host1(config-if)#lacp passive

`

The following commands add the Ethernet physical interfaces to a LAG bundle named chicago.

`

host1(config)#interface lag chicago
host1(config-if)#member-interface fastEthernet 4/0
host1(config-if)#member-interface fastEthernet 4/3

`

The following commands configure a PPPoE subinterface for the LAG bundle named chicago. In the LAG interface identification command (interface lag chicago.1), the number 1 represents the subinterface number for the PPPoE subinterface.

`

host1(config-if)#encapsulation pppoe
host1(config)#interface lag chicago.1
host1(config-if)#encapsulation ppp
host1(config-if)#ip address 10.10.1.1 255.255.0.0

`

As an alternative to using the command interface lag chicago.1 to configure the PPPoE subinterface in this example, you can also use the command pppoe subinterface lag chicago.1 to achieve the same result. For more information, see pppoe subinterface lag.

[Contents] [Prev] [Next] [Index] [Report an Error]