[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Interfaces and Policy Lists

#### Purpose

Display information about an interface and its policy lists. The delta keyword displays baselined statistics and the brief keyword displays the operational status of all configured interfaces

#### Action

To display information about interfaces and policy lists:

    host1#show interfaces fastEthernet 1/0.1
    FastEthernet1/0.1 is Up, Administrative status is Up
      VLAN ID: 100

      In: Bytes 4156, Packets 30
       Errors 0, Discards 0
      Out: Bytes 6406, Packets 45
       Errors 0, Discards 0

    VLAN policy input vlanPol1
      classifier-group vlan20 entry 1
        5 packets, 730 bytes
        filter

    host1#show ip interfaces atm 5/0.2
    ATM5/0.2 line protocol Atm1483 is down, ip is down (ready)
      Network Protocols: IP
      Internet address is 2.2.2.2/255.255.255.255
      Broadcast address is 255.255.255.255
      Operational MTU = 0  Administrative MTU = 0
      Operational speed = 100000000  Administrative speed = 0
      Discontinuity Time = 0
      Router advertisement = disabled
      Proxy Arp = disabled
      Network Address Translation is disabled
      TCP MSS Adjustment = disabled
      Administrative debounce-time = disabled
      Operational debounce-time    = disabled
      Access routing = disabled
      Multipath mode = hashed
      Auto Configure = disabled
      Auto Detect = disabled
      Inactivity Timer = disabled

      In Received Packets 0, Bytes 0
        Unicast Packets 0, Bytes 0
        Multicast Packets 0, Bytes 0
      In Policed Packets 0, Bytes 0
      In Error Packets 0
      In Invalid Source Address Packets 0
      In Discarded Packets 0
      Out Forwarded Packets 0, Bytes 0
        Unicast Packets 0, Bytes 0
        Multicast Routed Packets 0, Bytes 0
      Out Scheduler Dropped Packets 0, Bytes 0
      Out Policed Packets 0, Bytes 0
      Out Discarded Packets 0

      IP policy input P
        classifier-group data entry 1
          0 packets, 0 bytes
          rate-limit-profile rlpData
               committed rate: 10000 bps, committed burst: 8192 bytes (default)
               peak Rate: 100000 bps, peak burst: 1875 bytes
            committed: 0 packets, 0 bytes, action: transmit
            conformed: 0 packets, 0 bytes, action: transmit
            exceeded:  0 packets, 0 bytes, action: drop
        classifier-group voice entry 1
          0 packets, 0 bytes
          rate-limit-profile rlpVoice
               committed rate: 64000 bps, committed burst: 100000 bytes (default)
               peak Rate: 100000 bps, peak burst: 1875 bytes
            committed: 0 packets, 0 bytes, action: transmit
            conformed: 0 packets, 0 bytes, action: transmit
            exceeded:  0 packets, 0 bytes, action: drop
        classifier-group video entry 1
          0 packets, 0 bytes
          rate-limit-profile rlpVideo
               committed rate: 70000 bps, committed burst: 875 bytes
               peak Rate: 100000 bps, peak burst: 1875 bytes
            committed: 0 packets, 0 bytes, action: transmit
            conformed: 0 packets, 0 bytes, action: transmit
            exceeded:  0 packets, 0 bytes, action: drop
      IP policy output P
        classifier-group data entry 1
          0 packets, 0 bytes
          rate-limit-profile rlpData
               committed rate: 20000 bps, committed burst: 150 bytes
               peak Rate: 200000 bps, peak burst: 3750 bytes
            committed: 0 packets, 0 bytes, action: transmit
            conformed: 0 packets, 0 bytes, action: transmit
            exceeded:  0 packets, 0 bytes, action: drop
        classifier-group voice entry 1
          0 packets, 0 bytes
          rate-limit-profile rlpVoice
               committed rate: 64000 bps, committed burst: 100000 bytes
               peak Rate: 200000 bps, peak burst: 3750 bytes
            committed: 0 packets, 0 bytes, action: transmit
            conformed: 0 packets, 0 bytes, action: transmit
            exceeded:  0 packets, 0 bytes, action: drop
        classifier-group video entry 1
          0 packets, 0 bytes
          rate-limit-profile rlpVideo
               committed rate: 140000 bps, committed burst: 850 bytes
               peak Rate: 200000 bps, peak burst: 3750 bytes
            committed: 0 packets, 0 bytes, action: transmit
            conformed: 0 packets, 0 bytes, action: transmit
            exceeded:  0 packets, 0 bytes, action: drop

#### Meaning

Table 32 lists the show interfaces command output fields.

Table 32: show interfaces Output Fields

Field Name | Field Description
--- | ---
Subinterface number | Location of the subinterface that carries the VLAN traffic
Administrative status | Operational state that you configured for this interface: up or down
VLAN ID | Domain number of the VLAN
In Bytes | Number of bytes received on the VLAN subinterface
In Packets | Sum of all unicast, broadcast, and multicast packets received on the VLAN or S-VLAN subinterface
In Errors | Value is always 0 (zero)
In Discards | Value is always 0 (zero)
Out Bytes | Number of bytes sent on the VLAN or stacked VLAN (S-VLAN) subinterface
Out Packets | Number of packets sent on the VLAN or S-VLAN subinterface
Out Errors | Value is always 0 (zero)
Out Discards | Value is always 0 (zero)
VLAN policy | Type and name of the VLAN policy

#### Related Topics

- show interfaces

[Contents] [Prev] [Next] [Index] [Report an Error]