[Contents] [Prev] [Next] [Index] [Report an Error]

# radius dynamic-request server

#### Syntax

[ no ] radius dynamic-request server ipAddress

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the IP address of a RADIUS dynamic-request server and puts the E-series router into RADIUS Configuration mode. The no version deletes the instance of the RADIUS server.

| Note: The radius dynamic-request server command replaces the functionality of the radius disconnect client command. The RADIUS Disconnect Configuration mode is deprecated. Use the radius dynamic-request server command to enter RADIUS Configuration mode and configure options formerly available in RADIUS Disconnect Configuration mode.

#### Options

- ipAddress—IP address of the server

#### Mode

Global Configuration

#### Related Topics

- Configuring RADIUS-Based Mirroring

[Contents] [Prev] [Next] [Index] [Report an Error]