[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Included RADIUS Attributes

#### Purpose

Display the RADIUS attributes that are included in and excluded from Acct-On, Acct-Off, Access-Request, Acct-Start, and Acct-Stop messages.

#### Action

To display the list of included RADIUS attributes:

    host1# show radius attributes-included
                                   Account   Account    Access    Account    Account
          Attribute Name             On        Off     Request     Start       Stop
    --------------------------     -------   -------   --------   --------   --------
    acct-authentic                 enabled   enabled   n/c        n/c        n/c
    acct-delay-time                enabled   enabled   n/c        n/c        n/c
    acct-link-count                n/c       n/c       n/c        enabled    enabled
    acct-multi-session-id          n/c       n/c       disabled   enabled    enabled
    acct-session-id                enabled   enabled   enabled    n/c        n/c
    acct-terminate-cause           n/c       enabled   n/c        n/c        n/c
    acct-tunnel-connection         n/c       n/c       enabled    enabled    enabled
    ascend-num-in-multilink        n/c       n/c       disabled   disabled   disabled
    called-station-id              n/c       n/c       enabled    enabled    enabled
    calling-station-id             n/c       n/c       enabled    enabled    enabled
    class                          n/c       n/c       n/c        enabled    enabled
    connect-info                   n/c       n/c       enabled    enabled    enabled
    dhcp-options                   n/c       n/c       disabled   disabled   disabled
    dhcp-mac-address               n/c       n/c       disabled   disabled   disabled
    dhcp-gi-address                n/c       n/c       disabled   disabled   disabled
    dsl-forum-attributes           n/c       n/c       disabled   disabled   disabled
    egress-policy-name(vsa)        n/c       n/c       n/c        enabled    enabled
    event-timestamp                enabled   enabled   n/c        enabled    enabled
    framed-compression             n/c       n/c       n/c        enabled    enabled
    framed-interface-id            n/c       n/c       n/c        disabled   disabled
    framed-ip-address              n/c       n/c       n/c        enabled    enabled
    framed-ip-netmask              n/c       n/c       n/c        enabled    enabled
    framed-ipv6-prefix             n/c       n/c       n/c        disabled   disabled
    ingress-policy-name(vsa)       n/c       n/c       n/c        enabled    enabled
    input-gigapkts(vsa)            n/c       n/c       n/c        n/c        enabled
    input-gigawords                n/c       n/c       n/c        n/c        enabled
    interface-description          n/c       n/c       enabled    enabled    enabled
    l2c-downstream-data(vsa)       n/c       n/c       disabled   disabled   disabled
    l2c-upstream-data(vsa)         n/c       n/c       disabled   disabled   disabled
    l2cd-acc-loop-cir-id(vsa)      n/c       n/c       disabled   disabled   disabled
    l2cd-acc-aggr-cir-id-bin(vsa)  n/c       n/c       disabled   disabled   disabled
    l2cd-acc-aggr-cir-id-asc(vsa)  n/c       n/c       disabled   disabled   disabled
    l2cd-act-data-rate-up(vsa)     n/c       n/c       disabled   disabled   disabled
    l2cd-act-data-rate-dn(vsa)     n/c       n/c       disabled   disabled   disabled
    l2cd-min-data-rate-up(vsa)     n/c       n/c       disabled   disabled   disabled
    l2cd-min-data-rate-dn(vsa)     n/c       n/c       disabled   disabled   disabled
    l2cd-att-data-rate-up(vsa)     n/c       n/c       disabled   disabled   disabled
    l2cd-att-data-rate-dn(vsa)     n/c       n/c       disabled   disabled   disabled
    l2cd-max-data-rate-up(vsa)     n/c       n/c       disabled   disabled   disabled
    l2cd-max-data-rate-dn(vsa)     n/c       n/c       disabled   disabled   disabled
    l2cd-min-lp-data-rate-up(vsa)  n/c       n/c       disabled   disabled   disabled
    l2cd-min-lp-data-rate-dn(vsa)  n/c       n/c       disabled   disabled   disabled
    l2cd-max-interlv-delay-up(vsa) n/c       n/c       disabled   disabled   disabled
    l2cd-act-interlv-delay-up(vsa) n/c       n/c       disabled   disabled   disabled
    l2cd-max-interlv-delay-dn(vsa) n/c       n/c       disabled   disabled   disabled
    l2cd-act-interlv-delay-dn(vsa) n/c       n/c       disabled   disabled   disabled
    l2cd-dsl-line-state(vsa)       n/c       n/c       disabled   disabled   disabled
    l2cd-dsl-type(vsa)             n/c       n/c       disabled   disabled   disabled
    l2tp-ppp-disconnect-cause      n/c       n/c       n/c        n/c        disabled
    mlppp-bundle-name              n/c       n/c       enabled    enabled    enabled
    nas-identifier                 enabled   enabled   enabled    enabled    enabled
    nas-port                       n/c       n/c       enabled    enabled    enabled
    nas-port-id                    n/c       n/c       enabled    enabled    enabled
    nas-port-type                  n/c       n/c       enabled    enabled    enabled
    output-gigapkts(vsa)           n/c       n/c       n/c        n/c        enabled
    output-gigawords               n/c       n/c       n/c        n/c        enabled
    pppoe-description(vsa)         n/c       n/c       enabled    enabled    enabled
    profile-service-descr(vsa)     n/c       n/c       disabled   disabled   disabled
    tunnel-assignment-id           n/c       n/c       n/c        enabled    enabled
    tunnel-client-auth-id          n/c       n/c       enabled    enabled    enabled
    tunnel-client-endpoint         n/c       n/c       enabled    enabled    enabled
    tunnel-interface-id            n/c       n/c       disabled   disabled   disabled
    tunnel-medium-type             n/c       n/c       enabled    enabled    enabled
    tunnel-preference              n/c       n/c       n/c        enabled    enabled
    tunnel-server-attributes       n/c       n/c       disabled   disabled   disabled
    tunnel-server-auth-id          n/c       n/c       enabled    enabled    enabled
    tunnel-server-endpoint         n/c       n/c       enabled    enabled    enabled
    tunnel-type                    n/c       n/c       enabled    enabled    enabled

#### Meaning

Table 57 lists the show radius attributes-included command output fields.

Table 57: show radius attributes-included Output Fields

Field Name | Field Description
--- | ---
Attribute Name | Name of the RADIUS attribute
Account On | Include status of the attribute in Acct-On messages: enabled, disabled, not configurable (n/c)
Account Off | Include status of the attribute in Acct-Off messages: enabled, disabled, n/c
Access Request | Include status of the attribute in Access Request messages: enabled, disabled, n/c
Account Start | Include status of the attribute in Acct-Start messages: enabled, disabled, n/c
Account Stop | Include status of the attribute in Acct-Stop messages: enabled, disabled, n/c

#### Related Topics

- show radius attributes-included

[Contents] [Prev] [Next] [Index] [Report an Error]