[Contents] [Prev] [Next] [Index] [Report an Error]

# ip disable-forwarding

#### Syntax

[ no ] ip disable-forwarding

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Disables forwarding of packets on the SRP Ethernet interface to maintain router performance. The no version enables forwarding of packets on the SRP Ethernet interface. You see an error message if you try to set this command for interfaces other than the SRP Ethernet interface.

#### Mode

Interface Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]