[Contents] [Prev] [Next] [Index] [Report an Error]

# frame-relay fragment

#### Syntax

frame-relay fragment [ [ fragmentSize ] [ fragmentation-only ] | reassembly-only ]

no frame-relay fragment

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures fragmentation and reassembly for the map class created with the map-class frame-relay command. The no version stops fragmentation and/or reassembly on the subinterface.

#### Options

- fragmentSize—Maximum payload size of a fragment in bytes; a number in the range 16–8188; default value is 52
- fragmentation-only—Specifies fragmentation only
- reassembly-only—Specifies reassembly only

#### Mode

Map Class Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]