[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Chassis-Wide Routes Downloaded by RADIUS Route-Download Servers

#### Purpose

Display chassis-wide information about routes that are downloaded by RADIUS route-download servers.

Use the optional detail keyword to display more detailed information about the downloaded routes.

Use the optional start keyword to specify the first router context that you want to display in the output. For example, aaa:a2 specifies that the display shows a list of router contexts starting with VRF a2 in virtual router aaa.

#### Action

To display chassis-wide information about routes that are downloaded by RADIUS route-download servers:

    host1#show aaa route-download routes global
                                            Number
                                              of
    Virtual Router        VRF       Present Routes
    --------------- --------------- ------- ------
    aaa                             n       4
    aaa             a1              n       4
    default                         y       4
    default         d1              n       4

To display more detailed information about the downloaded routes:

    host1# show aaa route-download routes global detail

    Virtual Router   VRF  Present  Prefix/Length      Type       NextHop       Dst/Met  Intf   Tag
    ---------------  ---  -------  ---------------  --------  ---------------  -------  -----  ---
    aaa                   n        192.168.1.1/32   Access-P  255.255.255.255  0/2      null0  0
    aaa                   n        192.168.1.2/32   Access-P  255.255.255.255  0/2      null0  0
    aaa                   n        192.168.3.1/32   Access-P  255.255.255.255  0/2      null0  0
    aaa                   n        192.168.4.1/32   Access-P  255.255.255.255  0/2      null0  0
    aaa              a1   n        192.168.5.3/32   Access-P  255.255.255.255  0/2      null0  0
    aaa              a1   n        192.168.7.1/32   Access-P  255.255.255.255  0/2      null0  0
    aaa              a1   n        192.168.7.5/32   Access-P  255.255.255.255  0/2      null0  0
    aaa              a1   n        192.168.9.1/32   Access-P  255.255.255.255  0/2      null0  0
    default               y        192.168.22.1/32  Access-P  255.255.255.255  0/2      null0  0
    default               y        192.168.23.1/32  Access-P  255.255.255.255  0/2      null0  0
    default               y        192.168.24.1/32  Access-P  255.255.255.255  0/2      null0  0
    default               y        192.168.25.1/32  Access-P  255.255.255.255  0/2      null0  0
    default          d1   n        192.168.40.6/32  Access-P  255.255.255.255  0/2      null0  0
    default          d1   n        192.168.40.7/32  Access-P  255.255.255.255  0/2      null0  0
    default          d1   n        192.168.40.8/32  Access-P  255.255.255.255  0/2      null0  0
    default          d1   n        192.168.40.9/32  Access-P  255.255.255.255  0/2      null0  0

To specify the first router context that you want to display in the output:

    host1#show aaa route-download routes global start aaa:a2
                                            Number
                                              of
    Virtual Router        VRF       Present Routes
    --------------- --------------- ------- ------
    default                         y       4
    default         d1              n       4

#### Meaning

Table 16 lists the show aaa route-download routes global command output fields.

Table 16: show aaa route-download routes global Output Fields

Field Name | Field Description
--- | ---
Virtual Router | Name of the virtual router used to download the routes
VRF | Name of the VRF used to download the routes
Present | Routes have been downloaded; y (yes) or n (no) indicates if the router context has been created.
Number of Routes | Number of current downloaded routes
Prefix/Length | IP address prefix and mask information for downloaded routes
Type | Type of downloaded routes; Access-P indicates routes downloaded from the RADIUS route-download server
NextHop | IP address of the next hop
Dst/Met | Administrative distance and number of hops for the route
Tag | Tag assigned to downloaded routes
Intf | Interface type and specifier

#### Related Topics

- show aaa route-download routes global

[Contents] [Prev] [Next] [Index] [Report an Error]