[Contents] [Prev] [Next] [Index] [Report an Error]

## vrrp

#### Description

Virtual Router Redundancy Protocol

#### Emergency

None

#### Alert

None

#### Critical

NVS error; out of resources; unexpected error

#### Error

Virtual router ID (VRID) creation or modification failure; association addresses creation or modification failure

#### Warning Log

IP interface used by VRRP was removed; unexpected advertisement received from neighbor; invalid authentication detected; unable to get IP interface’s primary address

#### Notice Log

VRRP neighbor found

#### Info

State machine change

#### Debug

Management get, set, create, and remove

#### Filter

interface interfaceType interfaceSpecifier [ vrrpIdentifier ]

- interface—Logs events on a specific interface
- interfaceType—Type of interface for which you want to log events
- interfaceSpecifier—Location of interface in the appropriate format

  | Note: For information about interface types and specifiers, see Interface Types and Specifiers in JUNOSe Command Reference Guide.

- vrrpIdentifier—ID of the VRRP router for which you want to log events

[Contents] [Prev] [Next] [Index] [Report an Error]