> - Download PDFs
> - type

> # type

> #### Syntax

> To configure the RTR operation:

> [ no ] type rtrType protocol ipIcmpEcho destination
> [ source-ipaddr srcAddr | source interfaceType interfaceSpecifier ]

> To specify the L2TP tunnel type:

> type tunnelType

> no type

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> From RTR Configuration mode, configures an RTR operation. The no version removes the configured type from the operation and resets all configuration for an RTR index.

> | Note: You must configure the operation’s type before you can configure any other characteristics of the operation.

> From Domain Map Configuration and Tunnel Group Tunnel Configuration modes, specifies the L2TP tunnel type (RADIUS attribute 64, Tunnel-Type).

> #### Options

> - rtrType—One of the following types of operation:
>   - echo—Performs end-to-end operation only
>   - pathEcho—Discovers a path to the destination and echoes each device on the path
> - destination—IP address or an IP hostname or domain name
> - srcAddr—Source IP address
> - interfaceType—Interface type; see Interface Types and Specifiers
> - interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
> - tunnelType—L2TP tunnel type

> #### Mode

> Domain Map Configuration, RTR Configuration, Tunnel Group Tunnel Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.