[Contents] [Prev] [Next] [Index] [Report an Error]

# interface atm

#### Syntax

[ no ] interface atm interfaceSpecifier [ multipoint | point-to-point ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures an ATM interface or subinterface type. The no version removes the interface or subinterface.

| Note: On the OC3-2 GE APS I/O module, you can configure only OC3/STM1 ATM interfaces in ports 0 and 1. Port 2 is reserved for a Gigabit Ethernet interface.

#### Options

- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- multipoint—Specifies an NBMA subinterface
- point-to-point—Specifies an ATM interface or subinterface; default

#### Mode

Global Configuration, Interface Configuration

#### Related Topics

- Configuring an MPLS Pseudowire with VCC Cell Relay Encapsulation, Configuring Local ATM Cross-Connects with AAL5 Encapsulation, and Configuring MPLS LSPs for L2VPNs in the JUNOSe BGP and MPLS Configuration Guide

[Contents] [Prev] [Next] [Index] [Report an Error]