[Contents] [Prev] [Next] [Index] [Report an Error]

# Enabling ATM Cell Mode

When you configure a rate limit profile to account for ATM cell tax, the forwarding code calculates this information to determine the size of a frame instead of using only the frame size.

- Issue the atm-cell-mode command to account for the ATM cell tax in statistics and rate calculations:
  `
  host1(config-policy-list)#atm-cell-mode
  `

Use the show rate-limit-profile command to display the state of the mode.

#### Related Topics

- Monitoring Policy Management Overview
- atm-cell-mode
- show rate-limit-profile

[Contents] [Prev] [Next] [Index] [Report an Error]