[Contents] [Prev] [Next] [Index] [Report an Error]

## pppoe

#### Description

Point-to-Point over Ethernet layer

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

Error enabling control packet log

#### Warning Log

PPPoE interface or subInterface removed from NVS

#### Notice Log

PPPoE enabled; status change for subInterface

#### Info

Line module status change

#### Debug

None

#### Filter

interface interfaceType interfaceSpecifier

- interface—Logs PPP events for a specific interface
- interfaceType—Type of interface for which you want to log PPP events
- interfaceSpecifier—Location of interface in the appropriate format

  | Note: For information about interface types and specifiers, see Interface Types and Specifiers in JUNOSe Command Reference Guide.

[Contents] [Prev] [Next] [Index] [Report an Error]