[Contents] [Prev] [Next] [Index] [Report an Error]

# suspicious-control-flow-detection protocol low-threshold

#### Syntax

suspicious-control-flow-detection protocol protocolValue
low-threshold lowThresholdValue

no suspicious-control-flow-detection protocol protocolValue low-threshold

#### Release Information

Command introduced in JUNOSe Release 7.3.0.

#### Description

Sets the low threshold rate at which a suspicious flow becomes no longer suspicious for a specific protocol. The no version restores the default for a protocol, which is a protocol-dependent non-zero numeric value.

#### Options

- protocolValue—Name of the protocol
- lowThresholdValue—Threshold value in packets per second; 0 or a number in the range 1–32767; a value of zero means that a suspicious flow cannot change to the nonsuspicious state via a threshold; a flow can only become nonsuspicious via a backoff time; if the low threshold value is zero and the backoff time is zero, the flow can only be considered nonsuspicious if the rate (in packets per second) goes to zero

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]