[Contents] [Prev] [Next] [Index] [Report an Error]

# show ip tunnel-route

#### Syntax

show ip tunnel-route [ vrf vrfName ] [ destination [ ipMask ] [ detail ] ]
[ all ] [ protocol ] [ filter ]

#### Release Information

Command introduced in JUNOSe Release 7.1.0.

#### Description

Displays current state of the IPv4 tunnel routing table.

#### Options

- vrfName—Contents of the IPv4 tunnel routing table associated with a VRF
- destination—IP address or domain name of the host to show
- ipMask—IP mask of the specific address to show
- detail—Displays detailed information about the specific prefix
- all—Displays all routes in the IPv4 tunnel routing table inserted from all protocols, not just the best routes
- protocol—One of the following protocols for which you want to display the best route or all routes in the tunnel routing table; no routes are displayed if routes for the specified protocol are not present in the tunnel routing table

  | Note: Other protocol options are available in the CLI, but they are not applicable to the tunnel routing table.

  - bgp-tunnel—Displays the BGP tunnel routes in the tunnel routing table
  - ldp—Displays the LDP tunnel routes in the tunnel routing table
  - rsvp—Displays the RSVP tunnel routes in the tunnel routing table
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

[Contents] [Prev] [Next] [Index] [Report an Error]