[Contents] [Prev] [Next] [Report an Error]

# SRP-SE10G Module Combination (1-GB Memory)

> Line module label | SRP-SE10G
> I/O module label | SRP-SE I/O
> Number of I/O ports | 2
> Software release | First supported: 5.3.0 Final supported: Not applicable
> Description | 35 W Switch route processor for ERX-310 router only (10 Gbps)
> Type | Not applicable
> Capability | Ethernet (IEEE 802.3) 10/100Base-T RS-232
> Software features | Not applicable
> Model compatibility | ERX-310 router
> SRP module compatibility | SRP-SE10G
> Module redundancy support | Not applicable
> Cables and connectors | RJ-45 RS-232 (DB-9) See ERX Hardware Guide, Chapter 5, Cabling ERX Routers for more information.
> LEDs | See Module LEDs.
> Alarms, errors, and events | See Monitoring Modules in JUNOSe System Basics Configuration Guide, Chapter 6, Managing Modules.

[Contents] [Prev] [Next] [Report an Error]