[Contents] [Prev] [Next] [Index] [Report an Error]

# transform-set

#### Syntax

transform-set transform0
[ transform1 [ transform2 [ transform3 [ transform4 [ transform5 ] ] ] ] ]

no transform-set

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the transform set(s) that an IPSec transport connection can use to negotiate a transform algorithm. You can specify up to six transform algorithms. The no version resets the transform to the default, esp-3des-hmac-sha.

#### Options

- transform0 through transform5—AH or ESP transform; use the online Help to view available transforms

#### Mode

IPSec Transport Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]