[Contents] [Prev] [Next] [Report an Error]

# CT1 Module Combination

> Line module label | CT1
> I/O module label | CT1 FULL I/O
> Number of I/O ports | 24
> Software release | First supported: 1.1.0 Final supported: 7.3.x
> Description | 40 W Channelized T1
> Type | Non-ASIC
> Capability | DS1, DS0 HDLC Framing
> Software features | See ERX Module Guide, Appendix A, Module Protocol Support for information about the layer 2 and layer 3 protocols and applications that this module combination supports.
> Model compatibility | ERX-7xx models ERX-1410 router
> SRP module compatibility | SRP-5G SRP-5G+ SRP-10G
> Module redundancy support | 1:N redundancy
> Cables and connectors | RJ-48C 100–ohm connector Use shielded cables to maintain EMC compliance. The line interface unit supports multiple line buildouts. Signal strength is software controlled. The transmitted signal complies with ANSI T1.102-1993 Digital Hierarchy - Electrical Interfaces (1999) for cable lengths up to 201 m (660 feet). See ERX Hardware Guide, Chapter 5, Cabling ERX Routers for more information.
> LEDs | See ERX Module Guide, Appendix B, Module LEDs.
> Alarms, errors, and events | See Monitoring Interfaces in the Configuring Channelized T1 and Channelized E1 Interfaces chapter of the JUNOSe Physical Layer Configuration Guide for Release 8.0.x and earlier.

[Contents] [Prev] [Next] [Report an Error]