[Contents] [Prev] [Next] [Index] [Report an Error]

# ip dynamic-interface-prefix

#### Syntax

ip dynamic-interface-prefix [ vrf vrfName ] prefix

no ip dynamic-interface-prefix [ vrf vrfName ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the prefix for the names of dynamic shared IP interfaces created for overlapping BGP/MPLS VPNs. The no version restores the default prefix, dyn.

#### Options

- vrfName—Name of the VRF in which the shared interface is created; a string of 1–32 alphanumeric characters
- prefix—String of 1–10 alphanumeric characters

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]