[Contents] [Prev] [Next] [Index] [Report an Error]

# path ds3 snmp trap link-status

#### Syntax

[ no ] path pathChannel ds3 ds3Channel snmp trap link-status

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables SNMP link status processing for a DS3 signal. This command applies to a DS3 over channelized SONET interface. The no version disables SNMP link status processing on an interface.

#### Options

- pathChannel—Number, in the range 1–2147483648, that identifies the path
- ds3Channel—Number, in the range 1–3, that identifies the path

#### Mode

Controller Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]