[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring NAT

This section explains how to view NAT license information, NAT statistics, NAT translation entries, NAT address pool information, and NAT inside and outside rule settings.

## Displaying the NAT License Key

The show license nat command displays the NAT license key.

show license nat

- Use to display the NAT license key configured on the router.
- Example

      host1#show license nat
      Nat license is nat_license

- See show license.

## Displaying Translation Statistics

The show ip nat statistics command displays internal statistics that apply to NAT operation.

show ip nat statistics

- Use to display internal NAT statistics.
- Field descriptions
  - Last dynamic allocation failure—Completion level of any dynamic allocation failures; the number of times the router attempted dynamic allocation but reached the dynamic allocation entry limit
  - Current static translation entries
    - Inside Source Simple—Number of inside source simple static translations
    - Outside Source Simple—Number of outside source simple static translations
    - Inside Source Extended—Number of inside source extended static translations
    - Outside Source Extended—Number of outside source extended static translations
  - Dynamic Translation Type—Type of dynamic translation (inside source simple, outside source simple, inside source extended )
  - Current—Current number of dynamic translations of the associated translation type
  - Peak—Peak number of dynamic translations of the associated translation type
  - Accumulated—Accumulated number of dynamic translations of the associated type; this value reflects the accumulation of dynamic translations since the last router reboot operation
  - Failed—Total number of installation attempts that failed for an associated translation type
  - Forwarding statistics for packets received on inside or outside interfaces
    - forwarded directly—Number of packets forwarded directly (that is, without the need of translation)
    - forwarded through translator—Number of packets forwarded through the NAT translator
    - discarded—Number of packets discarded immediately upon receipt
    - discarded by translator—Number of packets discarded by the NAT translator when no matching translation could be located
- Example

      host1#show ip nat statistics
      NAT database statistics for virtual router vr1:
      --------------------------------------------------------------
      Last dynamic allocation failure: normal, successful completion
      Dynamic entry limit was reached 10318 times

      Current static translation entries:
      -----------------------------------------
      Inside Source Simple:               10
      Outside Source Simple:              3
      Inside Source Extended:             8
      Outside Source Extended:            12

             Dynamic
         Translation Type      Current       Peak     Accumulated    Failed
      ----------------------  ----------  ----------  -----------  ----------
      Inside Source Simple         69999       69999        69999       12568
      Outside Source Simple         4518        4518         4518          25
      Inside Source Extended       70000       70000        70000         568
      Fully Extended               26855       26855        26855        2565

      Forwarding statistics for virtual router vr1:
      ------------------------------------------------------------------------
      Packets received on inside interface and
          forwarded directly             8
          forwarded through translator   111763104
          discarded                      2
          discarded by translator        28524565

      Bytes received on inside interface and
          forwarded directly             544
          forwarded through translator   5141098074

      Packets received on outside interface and
          forwarded directly             7
          forwarded through translator   1031624
          discarded                      3
          discarded by translator        578961

      Bytes received on outside interface and
          forwarded directly             476
          forwarded through translator   47454704

- See show ip nat statistics.

## Displaying Translation Entries

The show ip nat translations command displays current translations that reside in the translation table.

Simple translation entries appear with inside/outside and local/global address information. Extended entries appear with added protocol and port numbers (or query IDs).

Using verbose mode additionally provides the time since creation and time since last use for each translation entry.

show ip nat translations

- Use to display current translations that reside in the NAT translation table.
- Field descriptions
  - Prot—Protocol (TCP, UDP, ICMP, or GRE) for this translation entry; this field appears only for extended table entries
  - Inside local—Inside local IP address for this translation entry; this field also provides the port number, separated by a colon ( : ) for extended entries
  - Inside global—Inside global IP address for this translation entry; this field also provides the port number, separated by a colon ( : ) for extended entries
  - Outside global—Outside global IP address for this translation entry; this field also provides the port number, separated by a colon ( : ) for extended entries
  - Outside local—Outside local IP address for this translation entry; this field also provides the port number, separated by a colon ( : ) for extended entries
  - Time since creation—Amount of time elapsed since the translation entry appeared in the translation table
  - Time since last use—Amount of time elapsed since the translation entry was used
- Example 1

      host1# show ip nat translations

      Prot    Inside local    Inside global    Outside global  Outside local
      ----    -------------   --------------   --------------  ---------------
      GRE     13.1.2.1:*      20.0.0.1:*            ---               ---
      ICMP    13.1.2.2:4      20.0.0.2:4            ---               ---
      TCP     13.1.2.3:20     20.0.0.3:50           ---               ---

  | Note: Because they are not NAPT translations, port numbers for GRE translations appear as asterisks (*).

- Example 2

      host1# show ip nat translations verbose

                                                            Time       Time
            Inside      Inside    Outside       Outside     since      since
      Prot  local       global    global        local       creation   last use
      ---- ----------- ---------- -----------   ----------- ---------- --------
           20.0.0.3     30.0.0.3    ---         ---         00:04:50   00:00:01
           21.0.0.3     30.208.0.3  ---         ---         00:02:12   00:00:01
           21.0.0.4     30.208.0.4  ---         ---         00:02:12   00:00:01
           ---          ---         50.0.0.3    70.0.0.3    00:03:24   Never
           ---          ---         51.0.0.3    70.208.0.3  00:01:44   00:00:01
           ---          ---         51.0.0.4    70.208.0.4  00:01:44   00:00:01
      UDP  ---          ---         50.50.0.3:8 70.50.0.3:8 00:03:10   Never
                                    7           108
      UDP  22.0.0.4:63  30.224.0.3: ---         ---         00:02:12   00:00:01
                        4097
      UDP  22.0.0.3:63  30.224.0.3: ---         ---         00:02:12   00:00:01
                        4096
      TCP  ---          ---         50.50.0.3:8 70.50.0.3:8 00:03:10   Never
                                    0           008
      UDP  20.50.0.3:87 30.50.0.3:8 ---         ---         00:03:35   Never
                        108

- See show ip nat translations.

## Displaying Address Pool Information

The show ip nat pool command displays NAT address pool information. The command output displays configuration (mask and address ranges) of all address pools, unless you supply a specific pool name.

show ip nat pool

- Use to display NAT address pool information.
- Field descriptions
  - pool—Name of the address pool
  - netmask—Network prefix associated with the NAT address pool
  - prefix length—Prefix length associated with the NAT address pool
  - range—Address ranges used by this NAT address pool
- Example 1

      host1#show ip nat pool

      pool: pool1 netmask: 255.255.255.0  prefix length: 24
         range: 3.3.3.1 to 3.3.3.255
         range: 4.4.4.1 to 4.4.4.32

      pool: pool2 netmask: 255.255.255.0  prefix length: 24
         range: 1.1.1.1 to 1.1.1.24
         range: 2.2.2.1 to 2.2.2.55

- Example 2

      host1#show ip nat pool pool1
      pool: pool1 netmask: 255.255.255.0  prefix length: 24
         range: 3.3.3.1 to 3.3.3.255
         range: 4.4.4.1 to 4.4.4.32

- See show ip nat pool.

## Displaying Inside and Outside Rule Settings

The show ip nat inside rule and show ip nat outside rule commands display access list and pool usage for all dynamic translation rules configured for the virtual router. If you do not specify an access list, the output displays address pool associations for each of the access lists for either inside or outside translation rules in the virtual router. Specifying an access list filters the output to display only the address pool associated with the specified list.

show ip nat inside rule

- Use to display NAT access list and pool usage information for inside source translation rules.
- Field descriptions
  - access list name—Name of the access list
  - pool name—Name of the address pool
  - rule type—Type of rule assigned
- Example

      host1#show ip nat inside rule
      access list name: list1  pool name: poolA rule type: inside source
      access list name: list2  pool name: poolB rule type: inside source
      access list name: list3  pool name: poolC rule type: inside source overload

- See show ip nat inside rule.

show ip nat outside rule

- Use to display NAT access list and pool usage information for outside source translation rules.
- Field descriptions
  - access list name—Name of the access list
  - pool name—Name of the address pool
  - rule type—Type of rule assigned
- Example

      host1#show ip nat outside rule
      access list name: list4  pool name: poolD rule type: outside source

- See show ip nat outside rule.

[Contents] [Prev] [Next] [Index] [Report an Error]