[Contents] [Prev] [Next] [Index] [Report an Error]

# aaa tunnel password

#### Syntax

aaa tunnel password name

no aaa tunnel password

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the default tunnel password. If the tunnel password is not included in the tunnel attributes that are returned from the domain map or authentication server, the router uses the default password. The no version deletes the password.

#### Options

- name—Default tunnel password; a string of up to 32 characters

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]