[Contents] [Prev] [Next] [Index] [Report an Error]

# l2tp destination profile

#### Syntax

l2tp destination profile { profileName [ [ virtual-router vrName ]
ip address ipAddress ] | [ virtual-router vrName ] ip address ipAddress }

no l2tp destination profile { profileName |
[ virtual-router vrName ] ip address ipAddress }

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Creates or accesses a destination profile that defines the location of a LAC. The no version removes the L2TP destination profile.

#### Options

- profileName—Name of the L2TP destination profile
- vrName—Name of the virtual router to be used to reach the destination (that is, the LAC). If you do not specify a virtual router, the current virtual router context is used.
- ipAddress—IP address to be used to reach the destination

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]