[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuration Examples

To configure a T3 interface, start at the Global Configuration mode, and issue the following commands:

`

host1(config)#controller t3 0/1
host1(config-controll)#no shutdwon
host1(config-controll)#framing c-bit
host1(config-controll)#clock source internal module
host1(config-controll)#cablelength 220
host1#exit

`

To configure an E3 interface, use the controller e3 command in place of the controller t3 command.

To configure HDLC channels on a T3 serial interface, issue the following commands:

`

host1(config)#controller t3 10/0
host1(config-controll)#exit
host1(config)#interface serial 10/0
host1(config-subif)#encapsulation ppp
host1(config-subif)#ip address 192.32.10.2 255.255.255.0

`

To configure fractional T3 on an interface, issue the following commands:

`

host1(config)#controller t3 10/0
host1(config-controll)#dsu mode 0
host1(config-controll)#dsu bandwidth 10000
host1(config-controll)#scramble

`

[Contents] [Prev] [Next] [Index] [Report an Error]