[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Upper-Level Protocols over Ethernet

This section explains how to use the show commands to display the physical characteristics and the configured settings for Ethernet interfaces.

| Note: The E120 router and E320 router output for monitor and show commands is identical to output from other E-series routers, except that the E120 and E320 router output also includes information about the adapter identifier in the interface specifier (slot/adapter/port).

You can use various show commands to monitor upper-layer protocols. For more information, see:

- Configuring Point-to-Point Protocol over Ethernet
- Chapter Configuring IP in JUNOSe IP, IPv6, and IGP Configuration Guide
- Chapter Configuring MPLS in JUNOSe BGP and MPLS Configuration Guide

show interfaces fastEthernet

- Use to display the status of Fast Ethernet interfaces, VLAN subinterfaces, or S-VLAN subinterfaces.
- You can specify the following keywords:
  - delta—Specifies that baselined statistics are to be shown
  - brief—Displays the operational status of all configured interfaces
- Field descriptions
  - FastEthernet interfaceSpecifier—Status of the hardware on this interface
    - up—Hardware is operational
    - down—Hardware is not operational
  - Administrative status—Operational state that you configured for this interface
    - up—Interface is enabled
    - down—Interface is disabled
  - Hardware—Type of MAC device on this interface
  - Address—MAC address of the processor on this interface
  - MAU—Type of medium attachment unit (MAU) on the physical port:
    - 10BASE-T (10 Mbps)
    - 100BASE-TX (100 Mbps)
    - 100BASE-FX-MM (100 Mbps) with the distance appearing after the type
    - 100BASE-LX-SM (100 Mbps)
    - SFP (Empty)—SFPs that are empty
    - SFP (Non-compliant Juniper Part)—SFPs that are installed in the FE-8 I/O module and do not have a Juniper Networks part number programmed
  - MTU—Size of the MTU for this interface
    - Operational—Size of the largest packet processed
    - Administrative—Setting for MTU size that you specified
  - Duplex Mode—Duplex option for this interface
    - Operational—Duplex option currently used
    - Administrative—Setting for duplex that you specified
  - Speed—Line speed for this interface
    - Operational—Current rate at which packets are processed
    - Administrative—Setting for line speed
    - 5 minute input rate—Data rates based on traffic received in the last 5 minutes
    - 5 minute output rate—Data rates based on traffic sent in the last 5 minutes
  - In—Analysis of inbound traffic on this interface
    - Bytes—Number of bytes received in error-free packets
    - Unicast—Number of unicast packets received
    - Multicast—Number of multicast packets received
    - Broadcast—Number of broadcast packets received
    - Errors—Total number of errors in all received packets; some packets might contain more than one error
    - Discards—Total number of discarded incoming packets
    - Mac Errors—Number of incoming packets discarded because of MAC sublayer failures
    - Alignment—Number of incomplete octets received
    - CRC—Number of packets discarded because the checksum the router computed from the data does not match the checksum generated by the originating devices
    - Too Longs—Number of packets discarded because the size exceeded the MTU
    - Symbol Errors—Number of symbols received that the router did not correctly decode
  - Out—Analysis of outbound traffic on this interface
    - Bytes—Number of bytes sent
    - Unicast—Number of unicast packets sent
    - Multicast—Number of multicast packets sent
    - Broadcast—Number of broadcast packets sent
    - Errors—Total number of errors in all transmitted packets; some packets might contain more than one error
    - Discards—Total number of discarded outgoing packets
    - Mac Errors—Number of outgoing packets discarded because of MAC sublayer failures
    - Deferred—Number of packets that the router delayed sending because the line was busy. In half duplex mode, a high number of deferrals means the link is very busy with traffic from other stations. In full duplex mode, when the link is always available for transmission, this number is zero.
    - No Carrier—Number of packets sent when carrier sense was unavailable
  - Collisions—Analysis of the collisions that occurred
    - Single—Number of packets sent after one collision
    - Multiple—Number of packets sent after multiple collisions
    - Late—Number of packets aborted during sending because of collisions after 64 bytes
    - Excessive—Number of packets not sent because of too many collisions
  - ARP Statistics—Analysis of ARP traffic on this interface; In fields are for traffic received on the interface and Out fields are for traffic sent on the interface
    - ARP requests—Number of ARP requests
    - ARP responses—Number of ARP responses
    - Errors—Total number of errors in all ARP packets
    - Discards—Total number of discarded ARP packets
  - queue—Hardware packet queue associated with the specified traffic class and interface
    - Queue length—Length of the queue, in bytes
    - Forwarded packets, bytes—Number of packets and bytes that were forwarded on this queue
    - Dropped committed packets, bytes—Number of committed packets and bytes that were dropped
    - Dropped conformed packets, bytes—Number of conformed packets and bytes that were dropped
    - Dropped exceeded packets, bytes—Number of exceeded packets and bytes that were dropped
- Example—Displays the status of a Fast Ethernet interface

      host1:vr2#show interfaces fastEthernet 2/0
      FastEthernet2/0 is Up, Administrative status is Up
        Hardware is Intel 21440, address is 0090.1a10.0552
        MAU is 10BASE-T
        MTU: Operational 1518, Administrative 1518
        Duplex Mode: Operational Full Duplex, Administrative Auto Negotiate
        Speed: Operational 100 Mbps, Administrative Auto Negotiate

        5 minute input rate 0 bits/sec, 0 packets/sec
        5 minute output rate 0 bits/sec, 0 packets/sec

        In: Bytes 39256, Unicast 612
         Multicast 0, Broadcast 0
         Errors 0, Discards 0, Mac Errors 0, Alignment 0
         CRC 0, Too Longs 0, Symbol Errors 0
        Out: Bytes 4579036, Unicast 610
         Multicast 0, Broadcast 70932
         Errors 0, Discards 0, Mac Errors 0, Deferred 0, No Carrier 3
         Collisions: Single 0, Multiple 0, Late 0, Excessive 0
       ARP Statistics:
        In: ARP requests 0, ARP responses 0
         Errors 0, Discards 0
        Out: ARP requests 0, ARP responses 0
         Errors 0, Discards 0
      Administrative qos-shaping-mode: none
      Operational qos-shaping-mode: none

      queue 0: traffic class control, bound to FastEthernet2/0
        Queue length 0 bytes
        Forwarded packets 1, bytes 46
        Dropped committed packets 0, bytes 0
        Dropped conformed packets 0, bytes 0
        Dropped exceeded packets 0, bytes 0

- See show interfaces.

show interfaces gigabitEthernet

show interfaces tenGigabitEthernet

- Use to display the status of Gigabit Ethernet interfaces, 10-Gigabit Ethernet interfaces, VLAN subinterfaces, or S-VLAN subinterfaces.
- You can specify the following keywords:
  - delta—Specifies that baselined statistics are to be shown
  - brief—Displays the operational status of all configured interfaces
- Field descriptions
  - GigabitEthernet or tenGigabitEthernet interfaceSpecifier—Status of the hardware on this interface
    - up—Hardware is operational
    - down—Hardware is not operational
  - Administrative status—Operational state that you configured for this interface
    - up—Interface is enabled
    - down—Interface is disabled
  - Hardware—Type of MAC device on this interface
  - Address—MAC address of the processor on this interface
  - MAU—Type of medium attachment unit (MAU) on the primary and secondary physical ports:
    - SFP—1000BASE-LH, 1000BASE-SX, 1000BASE-ZX; for SFPs that are empty, SFP (Empty) appears in this field; for SFPs that are installed in the OC3-2 GE APS I/O module and do not have a Juniper Networks part number programmed, SFP (GE Compliant) appears in this field
    - XFP—10GBASE-SR (10 Gbps), 10GBASE-LR (10 Gbps), 10GBASE-ER (10 Gbps); for XFPs that are empty, XFP (Empty) appears in this field
  - MTU—Size of the MTU for this interface
    - Operational—Size of the largest packet processed
    - Administrative—Setting for MTU size that you specified
  - Duplex Mode—Duplex option for this interface
    - Operational—Duplex option currently used
    - Administrative—Setting for duplex that you specified
  - Speed—Line speed for this interface
    - Operational—Current rate at which packets are processed
    - Administrative—Setting for line speed that you specified
  - Link—Link information for this interface
    - Operational Link Selected—Port that the I/O module is currently using: primary or secondary
    - Administrative link selected—Port that the I/O module is configured to use:
      - primary—Only primary port is configured to operate
      - secondary—Only redundant port is configured to operate
      - automatically—Software controls port redundancy automatically
  - Primary link selected x times—Number of times that the I/O has used the primary port since the module was last rebooted
  - Secondary link selected x times—Number of times that the I/O has used the secondary port since the module was last rebooted
  - Primary/Secondary link signal detected, Primary/Secondary link signal not detected—Specifies the port (primary or secondary) on which the router detects a signal
  - 5 minute input rate—Data rates based on the traffic received in the last 5 minutes
  - 5 minute output rate—Data rates based on the traffic sent in the last 5 minutes
  - In—Analysis of inbound traffic on this interface
    - Bytes—Number of bytes received in error-free packets
    - Unicast—Number of unicast packets received
    - Multicast—Number of multicast packets received
    - Broadcast—Number of broadcast packets received
    - Errors—Total number of errors in all received packets; some packets might contain more than one error
    - Discards—Total number of discarded incoming packets
    - Mac Errors—Number of incoming packets discarded because of MAC sublayer failures
    - Alignment—Number of incomplete octets received
    - CRC—Number of packets discarded because the checksum that the router computed from the data does not match the checksum generated by the originating devices
    - Too Longs—Number of packets discarded because the size exceeded the MTU
    - Symbol Errors—Number of symbols received that the router did not correctly decode
  - Out—Analysis of outbound traffic on this interface
    - Bytes—Number of bytes sent
    - Unicast—Number of unicast packets sent
    - Multicast—Number of multicast packets sent
    - Broadcast—Number of broadcast packets sent
    - Errors—Total number of errors in all transmitted packets; note that some packets might contain more than one error
    - Discards—Total number of discarded outgoing packets
    - Mac Errors—Number of outgoing packets discarded because of MAC sublayer failures
    - Deferred—Number of packets that the router delayed sending because the line was busy. In half duplex mode, a high number of deferrals means the link is very busy with traffic from other stations. In full duplex mode, when the link is always available for transmission, this number is zero.
    - No Carrier—Number of packets sent when carrier sense was unavailable
  - Collisions—Analysis of the collisions that occurred
    - Single—Number of packets sent after one collision
    - Multiple—Number of packets sent after multiple collisions
    - Late—Number of packets aborted during sending because of collisions after 64 bytes
    - Excessive—Number of packets not sent because of too many collisions
  - ARP Statistics—Analysis of ARP traffic on this interface; In fields are for traffic received on the interface and Out fields are for traffic sent on the interface
    - ARP requests—Number of ARP requests
    - ARP responses—Number of ARP responses
    - Errors—Total number of errors in all ARP packets
    - Discards—Total number of discarded ARP packets
  - queue—Hardware packet queue associated with the specified traffic class and interface
    - Queue length—Length of the queue, in bytes
    - Forwarded packets, bytes—Number of packets and bytes that were forwarded on this queue
    - Dropped committed packets, bytes—Number of committed packets and bytes that were dropped
    - Dropped conformed packets, bytes—Number of conformed packets and bytes that were dropped
    - Dropped exceeded packets, bytes—Number of exceeded packets and bytes that were dropped
- Example—Displays the status of a Gigabit Ethernet interface

      host1:vr2#show interfaces gigabitEthernet 10/2
      ERX-40-20-43#show int gigabitEthernet 10/2
      GigabitEthernet10/2 is Down, Administrative status is Up
        Hardware is SEEQ 8101, address is 0090.1a01.0cc8
        Primary MAU is 1000BASE-SX, secondary MAU is SFP (Empty)
        MTU: Operational 1518, Administrative 1518
        Duplex Mode: Operational Full Duplex, Administrative Auto Negotiate
        Speed: Operational 1000 Mbps, Administrative Auto Negotiate
        Link: Operational Secondary Link Selected,
              Administrative Link Selected Automatically
        Link Failover Timeout: Operational 652 ms, Administrative default
        Primary link selected 6302 times, Secondary link selected 6302 times
        Primary link signal detected, Secondary link signal detected

        5 minute input rate 0 bits/sec, 0 packets/sec
        5 minute output rate 0 bits/sec, 0 packets/sec

        In: Bytes 0, Unicast 0
         Multicast 0, Broadcast 0
         Errors 0, Discards 0, Mac Errors 0, Alignment 0
         CRC 0, Too Longs 0, Symbol Errors 0
        Out: Bytes 0, Unicast 0
         Multicast 0, Broadcast 0
         Errors 0, Discards 0, Mac Errors 0, Deferred 0, No Carrier 0
         Collisions: Single 0, Multiple 0, Late 0, Excessive 0
       ARP Statistics:
        In: ARP requests 0, ARP responses 0
         Errors 0, Discards 0
        Out: ARP requests 0, ARP responses 0
         Errors 0, Discards 0
      Administrative qos-shaping-mode: none
      Operational qos-shaping-mode: none

      queue 0: traffic class control, bound to GigabitEthernet10/2
        Queue length 0 bytes
        Forwarded packets 0, bytes 0
        Dropped committed packets 0, bytes 0
        Dropped conformed packets 0, bytes 0
        Dropped exceeded packets 0, bytes 0

- See show interfaces.

[Contents] [Prev] [Next] [Index] [Report an Error]