[Contents] [Prev] [Next] [Index] [Report an Error]

# vlan bulk-config shutdown

#### Syntax

To shut down or reenable the specified bulk configuration or a specific VLAN range:

[ no ] vlan bulk-config bulkConfigName shutdown

[ no ] vlan bulk-config bulkConfigName shutdown vlan-range vlanIdStart vlanIdEnd

To shut down or reenable VLAN ranges containing double-tagged S-VLAN IDs or based on agent-circuit-identifier information:

[ no ] vlan bulk-config bulkConfigName shutdown svlan-range s-vlanIdStart s-vlanIdEnd
{ vlanIdStart vlanIdEnd | any | agent-circuit-identifier }

#### Release Information

Command introduced in JUNOSe Release 7.3.0.

#### Description

Administratively disables (shuts down) the specified bulk configuration, or a specified VLAN range or subrange. When you shut down a specified bulk configuration, all VLAN ranges, including those based on double-tagged S-VLAN IDs or agent-circuit-identifier information, are disabled. The no version reenables the specified bulk configuration, the specified VLAN range, or the specified subranges; this is the default condition.

#### Options

- bulkConfigName—Name of the VLAN range; string of up to 80 characters
- vlanIdStart—Starting VLAN ID of the VLAN subrange you are configuring
- vlanIdEnd—Ending VLAN ID of the VLAN subrange you are configuring
- s-vlanIdStart—Starting S-VLAN ID of the S-VLAN subrange you are configuring
- s-vlanIdEnd—Ending S-VLAN ID of the S-VLAN subrange you are configuring
- any—Specifies the VLAN ID as a wildcard
- agent-circuit-identifier—Specifies a VLAN range that is based on agent-circuit-identifier information

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]