[Contents] [Prev] [Next] [Index] [Report an Error]

# aaa intf-desc-format include

#### Syntax

aaa intf-desc-format include { sub-intf | adapter } { enable | disable }

no aaa intf-desc-format include { sub-intf | adapter }

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies whether the subinterface or adapter is included in or omitted from the interface description that the router passes to RADIUS for inclusion in the NAS-Port-Id attribute. Also affects the Interface field displayed by the show subscribers command. The no version restores the default, in which the subinterface and adapter are included.

#### Options

- sub-intf—Specifies that the subinterface is included in or omitted from the interface description
- adapter—Specifies that the adapter is included in or omitted from the interface description
- enable—Includes the subinterface or adapter in the interface description; this is the default
- disable—Omits the subinterface or adapter from the interface description

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]