[Contents] [Prev] [Next] [Index] [Report an Error]

# atm lbo

#### Syntax

atm lbo { long | short }

no atm lbo

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the cable length (line build-out) for the ATM T3 or E3 interface. The length of cable determines power requirements. The no version restores the default value.

#### Options

- long—Specifies cable length in the range 226–450 feet
- short—Specifies cable length in the range 0–225 feet (the default)

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]