[Contents] [Prev] [Next] [Index] [Report an Error]

# show frame-relay pvc

#### Syntax

show frame-relay pvc [ dlci | interface interfaceType interfaceSpecifier ]
[ brief ] [ delta ] [ filter ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Displays permanent virtual circuit statistics for Frame Relay or MLFR interfaces.

#### Options

- dlci—DLCI number to be used on the specified subinterface to identify a virtual circuit in the range 16–1007
- interfaceType—One of the following interface types listed in Interface Types and Specifiers :
  - serial
  - pos
  - mlframe-relay
  - tunnel—GRE tunnel
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- brief—Displays the abbreviated version of the command output
- delta—Displays baselined statistics
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

[Contents] [Prev] [Next] [Index] [Report an Error]