[Contents] [Prev] [Next] [Index] [Report an Error]

# mpls ldp vpls neighbor

#### Syntax

[ no ] mpls ldp vpls vplsName neighbor ipAddress

#### Release Information

Command introduced in JUNOSe Release 8.2.0.

#### Description

Configures the remote VPLS edge (VE) device address of a neighbor in the VPLS domain in which the VPLS instance participates. The specified VPLS instance must use LDP as the signaling protocol. If either or both LDP or MPLS are not configured on the current virtual router, issuing this command creates the LDP and MPLS configurations automatically. The no version deletes the neighbor from the VPLS domain.

The mpls ldp vpls neighbor command is not valid for a VPLS instance that uses BGP as the signaling protocol. To configure a VPLS instance with BGP signaling, use the bridge vpls rd, bridge vpls route-target, bridge vpls site-name site-id, and bridge vpls site-range commands.

#### Options

- vplsName—Name of a VPLS instance created with the bridge vpls transport-virtual-router command
- ipAddress—IP address of a neighbor in the VPLS domain

#### Mode

Global Configuration

#### Related Topics

- Configuring LDP Signaling for VPLS in the JUNOSe BGP and MPLS Configuration Guide

[Contents] [Prev] [Next] [Index] [Report an Error]