> - Download PDFs
> - show l2tp dial-out session

> # show l2tp dial-out session

> #### Syntax

> show l2tp dial-out session [ triggerIpAddress | allVirtualRouters ] [ detail ]
> [ state operState ] [ filter ]

> To display summary information:

> show l2tp dial-out session summary [ allVirtualRouters ] [ filter ]

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Displays the status of L2TP dial-out sessions.

> #### Options

> - triggerIpAddress—Trigger IP address for the session that you want to display
> - allVirtualRouters—Displays dial-out information for all virtual routers
> - detail—Displays configuration, state, and statistics
> - operState—One of the following operational states:
>   - authenticating
>   - connecting
>   - dormant
>   - failed
>   - inService
>   - inhibited
>   - pending
>   - postInhibited
> - filter—See Filtering show Commands
> - summary—Displays aggregate counts for dial-out sessions in each of the possible operational and administrative states

> #### Mode

> Privileged Exec

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.