[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Default Integrated Mode for ATM Interface

In the default integrated mode, the SAR scheduler is the dominant scheduler, and it backpressures the first-stage (HRR) scheduler per VC. Each VC buffers only a few hundred bytes.

Figure 44 shows the default integrated mode.

Figure 44: Default Integrated Mode

To configure default integrated mode:

1. From the desired port, set the QoS port mode to default integrated mode.
   `
   host1(config)#interface atm 2/0
   host1(config-if)#no qos-mode-port
   `

   | Tip: For ATM interfaces on ERX-7xx models, ERX-14xx models, and the ERX-310 router, you must specify port 0.

2. Specify the VP shaping rate.
   `
   host1(config-if)#atm vp-tunnel 0 2000
   `

   | Tip: Configuring an ATM VP tunnel sets a shaping rate in the SAR scheduler. Before configuring an ATM VP tunnel, there must be no PVCs with the same VPI that you are about to configure. Before using the atm vp-tunnel command, remove any PVCs from the configuration. You can reconfigure the PVCs after configuring the shapeless VP tunnel.

3. Specify the shaping rate for the ATM subinterface.
   `
   host1(config-if)#interface atm 2/0.5
   host1(config-subif)#atm-pvc 5 0 5 aal5snap 768
   `

#### Related Topics

- Per-Packet Queuing on the SAR Scheduler Overview
- Guidelines for Configuring QoS over ATM
- atm vp-tunnel command
- interface atm command
- qos-mode-port command

[Contents] [Prev] [Next] [Index] [Report an Error]