[Contents] [Prev] [Next] [Index] [Report an Error]

# ip debounce-time

#### Syntax

ip debounce-time [ vrf vrfName ] period

no ip debounce-time [ vrf vrfName ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Defines the minimum time an IP interface must be in a given state—for example, up or down—before being reported. The no version removes the debounce time.

#### Options

- vrfName—Name of the VRF; string of 1–32 alphanumeric characters
- period—Interval in the range 0–60000 milliseconds

#### Mode

Global Configuration, Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]