[Contents] [Prev] [Next] [Index] [Report an Error]

# bridge1483 service-profile

#### Syntax

[ no ] bridge1483 service-profile profileName

#### Release Information

Command introduced in JUNOSe Release 9.0.0.

#### Description

Assigns the specified IP service profile to the interface profile from which a dynamic bridged Ethernet interface is created. The IP service profile must be defined in the default virtual router. The no version removes the IP service profile assignment from the interface profile.

#### Options

- profileName—Name of the IP service profile; maximum of 32 alphanumeric characters

#### Mode

Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]