[Contents] [Prev] [Next] [Index] [Report an Error]

# baseline ppp interface

#### Syntax

baseline ppp interface { atm | mlppp | pos | serial } interfaceSpecifier

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets a statistics baseline for PPP interfaces. The router implements the baseline by reading and storing the statistics at the time the baseline is set and then subtracting this baseline whenever baseline-relative statistics are retrieved. There is no no version.

#### Options

- atm—Specifies an ATM interface
- mlppp—Specifies an MLPPP interface
- pos—Specifies a POS interface
- serial—Specifies a serial interface
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers

#### Mode

Privileged Exec

[Contents] [Prev] [Next] [Index] [Report an Error]