[Contents] [Prev] [Next] [Index] [Report an Error]

# Other Software Standards

Table 63: E-series Non-RFC Software Standards

Reference | Protocol or Feature
--- | ---
ANSI T1.107a-1990 Standard for Telecommunications—Digital Hierarchy – Supplement to Formats Specification (August 1990) | MDL (T3 interfaces)
ANSI T1.403-1989 Standard for Telecommunications—Network and Customer Installation Interfaces – DS1 Metallic Interface – Robbed-bit Signaling State Definitions (1989) | FDL (T1 interfaces)
ANSI T1.404-1994 Standard for Telecommunications—Network-to-Customer – DS3 Metallic Interface Specification (1994) | Remote loopback (T3 interfaces
ANSI T1.617 Annex D | Frame Relay
AT&T Technical Reference 54016—Requirements for Interfacing Digital Terminal Equipment to Services Employing the Extended Superframe Format (September 1989) | FDL (T1 interfaces)
ATM Forum—ATM User-Network Interface Specification, Version 3.0 (September 1993) | ATM
ATM Forum—ATM User-Network Interface Specification, Version 3.1 (September 1994) | ATM
ATM Forum—Integrated Local Management Interface (ILMI) Specifications, Versions 3.0, 3.1, and 4.0 (September 1996) | ATM
ATM Forum—Traffic Management Specification, Version 4.0 (April 1996) | ATM
ATM Forum—User-Network Interface (UNI) versions 3.0, 3.1, 4.0 | ATM
Draft Standard P802.1Q/D9 IEEE Standards for Local and Metropolitan Area Networks: Virtual Bridged Local Area Networks | Ethernet; VLANs; Transparent bridging
DSL Forum Technical Report (TR)-059—DSL Evolution - Architecture Requirements for the Support of QoS-Enabled IP Services | QoS; DSL
DSL Forum Technical Report (TR)-101—Migration to Ethernet-Based DSL Aggregation (April 2006) | Dynamic VLANs; PPPoE; DHCP
ERX system Cisco HDLC is compatible with Cisco Systems HDLC protocol | Cisco HDLC
Frame Relay Forum—Frame Relay Fragmentation Implementation Agreement, FRF.12 (December 1997) | Frame Relay
Frame Relay Forum—User-to-Network Implementation Agreement (UNI), FRF 1.1 (January 1996) | Frame Relay
IEEE 802.1D—Media access control (MAC) bridges | Transparent bridging
IEEE 802.1q (Virtual LANs) | Ethernet; VLANs
IEEE 802.1w (Rapid Reconfiguration of Spanning Tree) | Ethernet
IEEE 802.1x-2001—Port-Based Network Access Control | Wireless authentication
IEEE 802.3 (Fast Ethernet and Gigabit Ethernet) | Ethernet
IEEE 802.3ad (Link Aggregation) | Link Aggregation, Layer 2 over MPLS
IEEE 802.3ae (10-Gigabit Ethernet only) | 10-Gigabit Ethernet
IEEE 802.3u (Fast Ethernet only) | Ethernet
IEEE 802.3z (Gigabit Ethernet only) | Ethernet
ISO International Standard 8473-1:1993—Information technology – Protocol for providing the connectionless-mode network service | IS-IS
ISO International Standard 9542:1988 (E)—Information processing systems – Telecommunications and information exchange between systems – End System-to-Intermediate System Routing Exchange Protocol for use in conjunction with the protocol for providing the connectionless-mode network service (ISO 8473) | IS-IS
ISO/IEC 10589:1992—Information technology – Telecommunications and information exchange between systems – Intermediate System-to-Intermediate System Intra-Domain Routing Exchange Protocol for use in conjunction with the protocol for providing the connectionless-mode network service (ISO 8473) | IS-IS
ITU O.151—Error performance measuring equipment operating at the primary rate and above (October 1992) | BERT Patterns
ITU O.153—Basic parameters for the measurement of error performance at bit rates below the primary rate (October 1992) | BERT Patterns
ITU-T Draft Recommendation I.363 (AAL5 support) (January 1993) | ATM
ITU-T G.783—Characteristics Of Synchronous Digital Hierarchy (SDH) Multiplexing Equipment Functional Blocks: Annex A – Multiplex Section Protection (MSP) Protocol, Commands And Operation (1990) | SDH MSP redundancy
ITU-T Q.933 Annex A | Frame Relay
ITU-T Recommendation I.610—B-ISDN Operation and Maintenance Principles and Functions (February 1999) | ATM
ITU-T Recommendation Q.922, Integrated Services Digital Network (ISDN) Data Link Layer Specification for Frame Mode Bearer Services; Annex A (February 1992) | Frame Relay
ITU-T V.35: Data transmission at 48 kbit/s using 60-108 kHz group band circuits (October 1984 - now obsolete) | V.35
ITU-T X.21: Interface between Data Terminal Equipment and Data Circuit-terminating Equipment for synchronous operation on public data networks (September 1992) | X.21
Lawfully Authorized Electronic Surveillance (LAES) for IP Network Access, American National Standard for Telecommunications, version PTSC-LAES-2006-084R6 | Packet Mirroring
Multilink Frame Relay UNI/NNI Implementation Agreement, FRF.16 (April 2000) | Multilink Frame Relay
T1M1.3 Working Group—A Technical Report on Test Patterns for DS1 Circuits (November 1993) | BERT Patterns
Telcordia document GR-253—Synchronous Optical Network (SONET) Transport Systems: Common Generic Criteria, Revision 3 (September 2000) | SONET APS redundancy

[Contents] [Prev] [Next] [Index] [Report an Error]