[Contents] [Prev] [Next] [Index] [Report an Error]

# ip multicast ioa-packet-replication

#### Syntax

ip multicast ioa-packet-replication interfaceType interfaceSpecifier

no ip multicast ioa-packet-replication

#### Release Information

Command introduced in JUNOSe Release 7.3.0.

#### Description

Enables IPv4 hardware multicast packet replication on port 8 of a high-density Ethernet I/O module or IOA. The no version disables hardware multicast packet replication.

#### Options

- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]