[Contents] [Prev] [Next] [Index] [Report an Error]

# pppoe profile

#### Syntax

[ no ] pppoe profile [ bridgedEthernet | ip | ppp | pppoe | any ] profileName

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Assigns a profile to a static PPPoE major interface. The profile configuration is used to dynamically configure an upper bridged Ethernet, IP, PPP, and/or PPPoE interface. The no version removes the profile assignment from the interface.

#### Options

- bridgedEthernet—Specifies a bridged Ethernet encapsulation type to which the profile applies
- ip—Specifies an IP encapsulation type to which the profile applies
- ppp—Specifies a PPP encapsulation type to which the profile applies
- pppoe—Specifies a PPPoE encapsulation type to which the profile applies
- any—Specifies any autoconfigured encapsulation that does not have a specific profile assignment
- profileName—Profile name of up to 80 characters

#### Mode

Interface Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]