[Contents] [Prev] [Next] [Index] [Report an Error]

# ip multicast admission-bandwidth-limit

#### Syntax

[ no ] ip multicast admission-bandwidth-limit limitValue

#### Release Information

Command introduced in JUNOSe Release 7.1.0.

#### Description

Specifies multicast admission bandwidth (in kilobits per second) for a given interface. The no version removes the admission bandwidth limit.

#### Options

- limitValue—Maximum admission bandwidth (in kilobits per second) permitted on an interface; default value is 0, which disables the limit

#### Mode

Interface Configuration, Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]