[Contents] [Prev] [Next] [Index] [Report an Error]

# pppoe motm

#### Syntax

pppoe motm string

no pppoe motm

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Causes the PPPoE application to send a PADM message of the minute message. The no version disables the message.

The recipient of the message is determined by the mode from which the command is issued. From Privileged Exec mode the message is sent to all PPPoE clients connected to the router; from Interface Configuration mode the PADM message is sent to the client as it is configured (if connected); and from Profile Configuration mode the message is sent to the new client created when the profile is dynamically attached to an IP interface. The MOTM string is passed with no changes.

#### Options

- string—Message sent

#### Mode

Interface Configuration, Privileged Exec, Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]