[Contents] [Prev] [Next] [Index] [Report an Error]

## Packet Mirroring References

For more information about RADIUS-based packet mirroring, consult the following resources:

- RFC 3576—Dynamic Authorization Extensions to Remote Authentication Dial In User Service (RADIUS) (July 2003)
- Lawfully Authorized Electronic Surveillance (LAES) for IP Network Access, American National Standard for Telecommunications, version PTSC-LAES-2006-084R6

[Contents] [Prev] [Next] [Index] [Report an Error]