[Contents] [Prev] [Next] [Index] [Report an Error]

# terminal length

#### Syntax

terminal length value

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the number of lines on the current terminal screen for the current session. There is no no version.

#### Options

- value—Number for the screen length in the range 0–512. If 0, the router does not pause between screens of output. If not 0, the router pauses between screens.

#### Mode

Privileged Exec, User Exec

[Contents] [Prev] [Next] [Index] [Report an Error]