[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Shared IPv6 Interfaces

You can create multiple shared IPv6 interfaces over the same layer 2 logical interface—for example, atm 5/3.101—enabling more than one IPv6 interface to share the same logical resources.

For additional information about shared interfaces, see Configuring Shared IPv6 Interfaces .

To share IPv6 interfaces:

1. Create a layer 2 interface.
   `
   host1(config)#interface atm 5/3
   host1(config-if)#interface atm 5/3.101
   `
2. (Optional) Create a primary IPv6 interface.
   `
   host1(config-if)#ipv6 address 1::1/64
   host1(config-if)#exit
   `
3. Create the shared IPv6 interface.
   `
   host1(config)#interface ipv6 si0
   `
4. Associate the shared IPv6 interface with the layer 2 interface by the following method:
   `
   host1(config-if)#ipv6 share-interface atm 5/3.101
   `
5. To fully configure the shared interface, assign an address (or make the interface unnumbered).
   `
   host1(config-if)#ipv6 address 1::1/64
   `

interface ipv6

- Use to create an IPv6 interface for interface sharing.
- Use the specified name to refer to the shared IPv6 interface; you cannot use the layer 2 interface to refer to them, because the shared interface can be moved.
- Example
  `
  host1(config)#interface ipv6 si1
  `
- Use the no version to delete the IPv6 interface.
- See interface ipv6

ipv6 share-interface

- Use to specify the layer 2 interface used by a shared IPv6 interface. The command fails if the layer 2 interface does not yet exist. The command is not supported (that is, it fails) if you use an RSVP tunnel (for example, tunnel mpls:1) to identify the layer 2 interface.
- After creating the shared IPv6 interface, you can configure it as you do any other IPv6 interface.
- The shared interface is operationally up when the layer 2 interface is operationally up.
- You can create operational shared IPv6 interfaces in the absence of a primary IPv6 interface.
- Example
  `
  host1(config-if)#ipv6 share-interface atm 5/3.101
  `
- Use the no version to remove the association between the layer 2 interface and the shared IPv6 interface. You can delete shared and primary IPv6 interfaces independently.
- See ipv6 share-interface

[Contents] [Prev] [Next] [Index] [Report an Error]