[Contents] [Prev] [Next] [Index] [Report an Error]

## Example: Simple Shared Shaping for Ethernet

In a typical triple-play network configuration over Ethernet, individual subscribers are represented on the B-RAS by VLANs and DSLAMs by SVLANs. In this example, the provider shapes the subscriber aggregate of voice, video, and data to a single rate.

In this example, S-VLAN 0 has traffic in three traffic-class groups: the default group, the TC1 traffic class in the G1 group, and the TC2 traffic class in the G2 traffic-class group.

Figure 21: Hierarchical Simple Shared Shaping over Ethernet

In Figure 21, the S-VLANs labeled 1, 2, and 3 indicate the possible constituents for S-VLAN 0. The active constituents for the simple shared shaper are the three nodes for S-VLAN 0 in the three traffic-class groups.

| Note: This example uses QoS parameters to configure shared shaping.

1. Configure the traffic classes and traffic-class groups.
   `
   (config)#traffic-class tc1
   (config)#exit
   (config)#traffic-class tc2
   (config)#exit
   (config)#traffic-class-group g1
   (config-traffic-class-group)#traffic-class tc1
   (config-traffic-class-group)#exit
   (config)#traffic-class-group g2 extended
   (config-traffic-class-group)#traffic-class tc2
   (config-traffic-class-group)#exit
   `
2. Configure the parameter definitions.
   `
   (config)#qos-parameter-define vlan-g1-max-rate
   (qos-parameter-define)#controlled-interface-type vlan
   (qos-parameter-define)#instance-interface-type vlan
   (qos-parameter-define)#exit
   (config)#qos-parameter-define svlan-g1-max-rate
   (qos-parameter-define)#controlled-interface-type svlan
   (qos-parameter-define)#instance-interface-type svlan
   (qos-parameter-define)#instance-interface-type ethernet
   (qos-parameter-define)#exit
   (config)#qos-parameter-define vlan-max-rate
   (qos-parameter-define)#controlled-interface-type vlan
   (qos-parameter-define)#instance-interface-type vlan
   (qos-parameter-define)#instance-interface-type svlan
   (qos-parameter-define)#exit
   (config)#qos-parameter-define svlan-max-rate
   (qos-parameter-define)#controlled-interface-type svlan
   (qos-parameter-define)#instance-interface-type svlan
   (qos-parameter-define)#instance-interface-type ethernet
   (qos-parameter-define)#exit
   `
3. Configure the shared shaper by referencing parameter definitions in the shaping-rate command.
   `
   (config)#scheduler-profile vlan-be
   (config-scheduler-profile)#shared-shaping-rate vlan-max-rate simple
   (config-scheduler-profile)#exit
   (config)#scheduler-profile svlan-be
   (config-scheduler-profile)# shared-shaping-rate svlan-max-rate simple
   (config-scheduler-profile)#exit
   (config)#scheduler-profile svlan-g1
   (config-scheduler-profile)#shaping-rate svlan-g1-max-rate
   (config-scheduler-profile)#exit
   (config)#scheduler-profile vlan-g1
   (config-scheduler-profile)#shaping-rate vlan-g1-max-rate
   (config-scheduler-profile)#exit
   (config)#scheduler-profile svlan-g2
   (config-scheduler-profile)#shaping-rate svlan-max-rate % 50
   (config-scheduler-profile)#exit
   `
4. Configure the QoS profile.
   `
   (config)#qos-profile svlan-4.1
   (config-qos-profile)#vlan queue traffic-class best-effort
   (config-qos-profile)#vlan node scheduler-profile vlan-be
   (config-qos-profile)#svlan node scheduler-profile svlan-be
   (config-qos-profile)#vlan queue traffic-class tc1
   (config-qos-profile)#svlan node scheduler-profile svlan-g1 group g1
   (config-qos-profile)#svlan queue traffic-class tc2
   (config-qos-profile)#svlan node scheduler-profile svlan-g2 group g2
   (config-qos-profile)#ethernet group g2 scheduler-profile default
   `
5. Attach the QoS profile to the S-VLANs on Fast Ethernet interface 11/0.
   `
   (config)#interface fastEthernet 11/0
   (config-if)#svlan 0 qos-parameter svlan-max-rate 4000000
   (config-if)#svlan 0 qos-profile svlan-4.1
   (config-if)#encapsulation vlan
   (config-if)#exit
   (config)#interface fastEthernet 11/0.1
   (config-if)#svlan id 0 1
   (config-if)#ip address 1.2.1.1 255.255.255.0
   (config-if)#exit
   (config)#interface fastEthernet 11/0.2
   (config-if)#svlan id 0 2
   (config-if)#ip address 1.3.1.1 255.255.255.0
   (config-if)#exit
   `

#### Related Topics

- Configuring Simple Shared Shaping
- Simple Shared Shaping Overview

[Contents] [Prev] [Next] [Index] [Report an Error]