[Contents][Prev][Next][Report an Error]

# OCx/STMx ATM IOAs

Table 29: OCx/STMx ATM IOA

Protocol or Application | ES2–S1 OC3–8 STM1 ATM IOA | ES2–S1 OC12–2 STM4 ATM IOA
--- | --- | ---
Accepts traffic destined for GRE tunnels or DVMRP (IP-in-IP) tunnels | Yes | Yes
APS/MSP | No | No
ATM | Yes | Yes
BERT | No | No
BFD | Yes | No
BGP | Yes | Yes
BGP/MPLS VPNs | Yes | Yes
Bridged Ethernet | Yes | Yes
Bridged IP | Yes | Yes
Cisco HDLC | No | No
DHCP external server | Yes | Yes
DHCP local server | Yes | Yes
DVMRP and GRE support—access side | Yes | Yes
DVMRP and GRE support—server side | Yes (over shared tunnel server ports) | Yes (over shared tunnel server ports)
Dynamic interfaces | Yes | Yes
F4 OAM and F5 OAM (ATM administration) | Yes | Yes
FDL (facilities data link) | No | No
Firewall | No | No
Frame Relay | No | No
IEEE 802.3ad link aggregation | No | No
IP | Yes | Yes
IP multicast | Yes | Yes
IP reassembly for tunneled packets | Yes | Yes
IPSec | No | No
IPv6 | Yes | Yes
IPv6 multicast | Yes | Yes
IPv6 neighbor discovery | Yes | Yes
IS-IS | Yes | Yes
J-Flow Statistics | Yes | Yes
L2TP/IPSec | No | No
L2TP over MPLS | Yes | Yes
LAC support—access side | Yes | Yes
LAC support—peer side | Yes | Yes
LNS support—peer side | Yes | Yes
Local loopback | No | No
MDL (maintenance data link) | No | No
Mobile IP home agent | No | No
MPLS | Yes | Yes
Multilink Frame Relay | No | No
Multilink PPP | No | No
Network Address Translation (NAT) | No | No
NBMA (multipoint ATM) | No | No
OSPF | Yes | Yes
Packet Mirroring | Yes | Yes
Packet over SONET | No | No
PPP | Yes | Yes
PPPoE | Yes | Yes
Remote loopback | No | No
RIP | Yes | Yes
Subscriber interfaces (static) | Yes | Yes
Subscriber interfaces (dynamic) | Yes | Yes
Transparent bridging | Yes | Yes
Tunnel-server ports | Yes (shared only) | Yes (shared only)
Unified ISSU | Yes | Yes
VPLS (network interfaces) | Yes | Yes
VPLS (virtual core interfaces) | Yes | Yes
VRRP | No | No

[Contents][Prev][Next][Report an Error]