[Contents] [Prev] [Next] [Index] [Report an Error]

# distribute-list

#### Syntax

In Router Configuration mode:

[ no ] distribute-list accessListName { in | out } [ interfaceType interfaceSpecifier ]

In Remote Neighbor Configuration mode:

[ no ] distribute-list accessListName { in | out }

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the distribute list, an access list applied to incoming or outgoing RIP route updates. In Remote Neighbor Configuration mode, applies only to a RIP remote-neighbor interface. The no version removes the distribute list. An IP access list acts as a filter; refer to the access-list command for details.

#### Options

- accessListName—Name of the access list; string of up to 32 alphanumeric characters
- in—Applies the access list to incoming route updates
- out—Applies the access list to outgoing route updates
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers

#### Mode

Address Family Configuration, Remote Neighbor Configuration, Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]