[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring a B-RAS License

From Global Configuration mode, configure a B-RAS license:

`

host1(config)#license b-ras k3n91s6gvtj

`

B-RAS licenses are available in various sizes to enable subscriber access for up to one of the following maximum number of simultaneous active IP, LAC, and bridged Ethernet interfaces:

- 4000
- 8000
- 16,000
- 32,000
- 48,000

  | Note: To use a B-RAS license for 16,000 or more interfaces, each of your SRP modules must have 1 gigabyte (GB) of memory.

license b-ras

- Use to specify the B-RAS license.
- The license is a unique string of up to 15 alphanumeric characters.

  | Note: Acquire the license from Juniper Networks Customer Service or your Juniper Networks sales representative.

- You can purchase licenses that allow up to 2,000, 4,000, 8,000, 16,000, 32,000, or 48,000 simultaneous active IP, LAC, and bridged Ethernet interfaces.
- Example
  `
  host1(config)#license b-ras jwmR4k8D
  `
- Use the no version to disable the license.
- See license b-ras

[Contents] [Prev] [Next] [Index] [Report an Error]