[Contents] [Prev] [Next] [Index] [Report an Error]

# Required Tools, Wires, and Cables

Cabling your system takes only a few minutes. You need the following items and those listed in Table 6 for proper installation:

- 1/8-inch flathead screwdriver
- 3/8-inch wrench or 3/8-inch nut-driver
- No. 2 Phillips screwdriver
- Ground wires—We recommend a minimum of 6-AWG ground wire.
- Two #10 kep nuts (supplied) to connect the ground (earth) wire to the ground terminal.
- PDU wiring—We recommend a minimum of 4-AWG wire for the router with a dual stud terminal lug with 5/8-inch spacing.

Consider the distance from the connection point and the configuration of the system when determining the size of wire used.

See System Specifications for more information on router specifications.

Table 6: Required Cables

Connection | Port and Cable Used
--- | ---
Management connection between SRP IOA and the LAN | One 10/100Base-T Ethernet management port with an RJ-45 connector
Management connection between SRP IOA and a management console | One RS-232 port with a DB-9 connector for VT100 management access
Direct connections to IOAs | See the E120 and E320 Module Guide for specific IOA connector information

[Contents] [Prev] [Next] [Index] [Report an Error]