[Contents] [Prev] [Next] [Index] [Report an Error]

# authorization change

#### Syntax

[ no ] authorization change

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables the router to receive change-of-authorization messages, such as packet mirroring attributes and Service Manager attributes, from the RADIUS server. The no version restores the default, in which support for RADIUS-initiated change-of-authorization messages is disabled on the router.

#### Mode

RADIUS Configuration

#### Related Topics

- Configuring RADIUS-Based Mirroring

[Contents] [Prev] [Next] [Index] [Report an Error]