[Contents] [Prev] [Next] [Index] [Report an Error]

# ip share-nexthop

#### Syntax

ip share-nexthop ipAddress [ virtual-router vrName ]

no ip share-nexthop

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies that the shared IP interface dynamically tracks a next hop for the specified destination. The no version halts tracking of the next hop.

#### Options

- ipAddress—IP address of the destination for which the next hop is tracked
- vrName—Name of the virtual router for the next hop

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]